,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,UGR##OTHER##,Total lm##OTHER##,Total Watt##ELECTRICAL_WATTAGE##WATTS,Single spot Watt##ELECTRICAL_WATTAGE##WATTS,Screen##OTHER##,SPOT 2 - rotation 2##ANGLE##DECIMAL DEGREES,SPOT 2 - rotation 1##ANGLE##DECIMAL DEGREES,SPOT 1 - rotation 2##ANGLE##DECIMAL DEGREES,SPOT 1 - rotation 1##ANGLE##DECIMAL DEGREES,Produttore##OTHER##,Modello##OTHER##,Lampada##OTHER##,Initial intensity##ELECTRICAL_LUMINOUS_FLUX##LUMENS,IP##OTHER##,Energy class##OTHER##,Commenti sul tipo##OTHER##,CRI##OTHER##,Body width##LENGTH##MILLIMETERS,Body length##LENGTH##MILLIMETERS,Body lamp##OTHER##,Body height##LENGTH##MILLIMETERS
91AA23L366,230.000000000000,https://www.esse-ci.com/product/scout/?,<22,374 lm,6.000000000000,3.000000000000,Spot with 35° beam angle,90.000000000000,90.000000000000,90.000000000000,90.000000000000,esse-ci,SCOUT SPOT/AA 2x3W 3000K 35° IP66,LED,187.000000000000,66,A+,© / esse-ci / We reserve the right to make technical changes without prior notice.,>80,24.999999999986,109.999999999989,Aluminum Scout spot,600.000000000000
91AA23L3L66,230.000000000000,https://www.esse-ci.com/product/scout/?,<22,374 lm,6.000000000000,3.000000000000,Spot with 35° beam angle,90.000000000000,90.000000000000,90.000000000000,90.000000000000,esse-ci,SCOUT SPOT/AA 2x3W 3000K 35° Long IP66,LED,187.000000000000,66,A+,© / esse-ci / We reserve the right to make technical changes without prior notice.,>80,24.999999999986,109.999999999989,Aluminum Scout spot,900.000000000000
